### Ssystem()

LONG Ssystem( mode, arg1, arg2)

WORD mode;
LONG arg1;
LONG arg2;

| Ssystem() is a multipurpose call controlling Cookie Jar, memory access and various system settings.
Opcode | 340 (0x0154)
Availability | Available when a 'MiNT' cookie with a version of at least 1.15 exists.
Parameters | arg1 and arg2 are long parameters specific for a particular mode. If a mode doesn't use a parameter, it is usually ignored, but should be set to a zero for future compatibility. mode specifies a particular action as follows:
| mode | meaning
| S_OSNAME (0x0000) | Identifies the operating system type. Returned longword contains a 32-bit positive number, which interpreted as an ASCII string gives a 4-character id. For MiNT the returned value is 0x4d694e54 ('MiNT').
| S_OSXNAME (0x0001) | Identifies the subtype of the operating system. If this call returns a zero or a negative value, that means, that no subtype is available. Otherwise the returned value, when interpreted as an ASCII string gives a 4-character subtype id. For FreeMiNT, being a derivative of the MiNT, the returned value is 0x46726565 ('Free'). If a subtype id is less than 4 characters long, it should be padded with zeros.
| S_OSVERSION (0x0002) | Identifies the exact operating system version. Returned longword contains a 32 bit positive version number encoded as follows:
    bits	meaning
    ----	-------
    0-7	some printable character
    	to characterize the current version,
    	e.g.
    	0x61 (`a') if alpha release,
    	0x62 (`b') if beta release.
    	For official releases you will
    	always find a value of 0 here.
    8-15	patchlevel (0x55 for pl 88)
    16-23	minor version number (0x0e for x.14)
    24-31	major version number ($01 for 1.xx)
Definition of an official release: every release for which in bits 0-7 a value of 0 is returned...
| S_OSHEADER (0x0003) | Allows to access the TOS header in order to get some information from. Current implementation allows to access the first 256 longwords of the header. The address of the required longword, relative to the begin address of the TOS header, has to be specified as arg1. Only even values are allowed (bit 0 of the arg1 is masked out by the kernel). Always a whole longword is returned.
| S_OSBUILDDATE (0x0004) | Returns a 32 bit positive value with the build date encoded as follows:
    bits	meaning
    ----	-------
    0-15	binary year ($07dd for 1998)
    16-23	binary month ($0c for the December)
    24-31	binary day of the month
| S_OSBUILDTIME (0x0005) | Returns a 32 bit positive value with the build time encoded as follows:
    bits	meaning
    ----	-------
    0-7	binary seconds
    8-15	binary minutes
    16-23	binary hours
    24-31	day of week
day of week has 1 for Monday, 2 for Tuesday... 7 for Sunday. The call should never return a zero in these bits, but if it does, it should be interpreted as Sunday.
| S_OSCOMPILE (0x0006) | Returns a 32-bit positive value specifying the primary CPU type the kernel has been compiled for. Encoding:
    bits	meaning
    ----	-------
    0-7	binary minor CPU ID
    8-15	binary major CPU ID
    16-31	reserved for future definition.
The major ID identifies a particular series of processors. Currently only a value of $00 is defined and it is assigned to Motorola 68k series. Other values of this field are reserved for future definition. The minor CPU ID interpretation depends on the major ID. For 68k series, values are as follows:
    $00	68000
    $0a	68010
    $14	68020
    $1e	68030
    $28	68040
    $3c	68060
This is not the same as the _CPU cookie value. The _CPU cookie specifies the CPU physically present in the machine, while the S_OSCOMPILE indicates the processor type selected at the time when the system was compiled. In other words, running a 68000 compiled kernel will return a $00 here, even if the machine is running 68040 or something.
| S_OSFEATURES (0x0007) | Returns a 32-bit positive value specifying the state of kernel features. Encoding:
    bits	meaning
    ----	-------
    0	memory protection (1 = turned on)
    1	virtual memory (1 = turned on)
    2-31	reserved for future usage
This call has an informative purpose only and you cannot toggle anything with it.
| S_GETCOOKIE (0x0008) | Fetches required information from the Cookie Jar. If arg1 is a value bigger than 65535 (0xffff), it is interpreted as a tag id. The Cookie Jar is searched for such a tag, then if the tag is found, the corresponding slot value is returned or -1 otherwise. If arg1 is a value between 1 and 65535, it is interpreted as a slot number, not a tag id.Then the corresponding tag id is fetched and returned or a value of -1 if the specified slot is free or does not exist at all (a slot number past the end of the Cookie Jar was specified). The first slot in the Cookie Jar is considered number 1. If arg1 is equal to a zero, then the Cookie Jar is searched for the NULL cookie, then the corresponding slot value is returned. The place where the value fetched from the Cookie Jar will be returned is defined by the arg2. If this is a zero, the call returns its values in the GEMDOS return value (d0). If the arg2 is not a zero, it is interpreted as a pointer to a memory location, where the slot tag or its value should be written to. The return value is 0 (E_OK) then, if everything went OK, or -1 otherwise. This behaviour (where arg2 != NULL) is not implemented in MiNT versions below 1.14.8.
| S_SETCOOKIE (0x0009) | Places a tag id specified by the arg1 with the value of the arg2 in the Cookie Jar. If a slot with the specified tag id already exists, it will be replaced with the new value. NULL cookie is reallocated automatically and its value is adjusted. If there are no more free slots, no action is performed and ENOMEM is returned instead. S_SETCOOKIE requires root euid, EACCES is returned otherwise and no action is performed. The call refuses to place a cookie (a value of -1 is returned) whose tag id contains a zero-byte.
| S_GETLVAL (0x000a) | Fetches and returns a longword from the address of supervisor area specified as a 16-bit, even, unsigned integer value passed as arg1. Bit 0 and bits 16-31 are masked out (ignored). The call returns a zero if the value at the specified address has to be "hidden" from reading. Currently the hidden values are the initial PC value and the initial stack pointer value stored at $00000000 and $00000004 respectively. Reading a hidden value may require root euid. If the desired address is long word aligned, longwords can be also retrieved from the supervisor area using Setexc().
| S_GETWVAL (0x000b) | Fetches and returns a word from the address of supervisor area specified as a 16-bit, even, unsigned integer value passed as arg1. Bit 0 and bits 16-31 are masked out (ignored). The call returns a zero if the value at the specified address has to be "hidden" from reading. Currently the hidden values are the initial PC value and the initial stack pointer value stored at $00000000 and $00000004 respectively. Reading a hidden value may require root euid.
| S_GETBVAL (0x000c) | Fetches and returns a byte from the address of supervisor area specified as a 16-bit unsigned integer value passed as arg1. Bits 16-31 are masked out (ignored). The call returns a zero if the value at the specified address has to be "hidden" from reading. Currently the hidden values are the initial PC value and the initial stack pointer value stored at $00000000 and $00000004 respectively. Reading a hidden value may require root euid.
| S_SETLVAL (0x000d) | Places a longword value specified by arg2 at address specified as 16 bit integer by arg1. Bit 0 and bits 16-31 of the arg1 are masked out (ignored). Since this call is designed to manipulate operating system variables located within the supervisor area (first 32k), it is restricted for root euid and returns EACCES if called by an unprivileged process.
| S_SETWVAL (0x000e) | Places a word value specified by arg2 at address specified as 16 bit integer by arg1. Bit 0 and bits 16-31 of the arg1 are masked out (ignored). Since this call is designed to manipulate operating system variables located within the supervisor area (first 32k), it is restricted for root euid and returns EACCES if called by an unprivileged process.
| S_SETBVAL (0x000f) | Places a byte value specified by arg2 at address specified as 16 bit integer by arg1. Bits 16-31 of the arg1 are masked out (ignored). Since this call is designed to manipulate operating system variables located within the supervisor area (first 32k), it is restricted for root euid and returns EACCES if called by an unprivileged process.
| S_SECLEVEL (0x0010) | Resets the current security level to a value specified by arg1. Valid levels are as follows: 0: none of hardware specific system calls are restricted. This is a 'MultiTOS compatibility' mode. 1: BIOS and XBIOS calls require root privileges; any call except Supexec() and Super() returns EACCES if called by an unprivileged process. This does not apply to Setexc(), which sends SIGSYS to the caller if a change of an exception vector was attempted. 2: as above, with except that Supexec() and Super() generates SIGSYS in order to kill the calling process. On values bigger than a 2, the EACCES is returned. If arg1 is equal to a -1, the current security level value is returned. The call totally needs root privileges - user processes cannot even inquire the current security level value.
| S_RUNLEVEL (0x0011) | Reserved for future definition.
| S_TSLICE (0x0012) | Allows to set/interrogate the global timeslice value. Values are exactly the same as for SLICES keyword in mint.cnf. If arg1 is equal to -1, the call returns the current global timeslice value. Setting the timeslice requires root privileges.
| S_FORCEFASTLOAD (0x0013) | Allows to change the interpretation of the FASTLOAD bit in the program header. On Ssystem(S_FORCEFASTLOAD, 0L, 0L); the program header bit will be used as before, this is actually equal to FASTLOAD=NO in mint.cnf. On Ssystem(S_FORCEFASTLOAD, 1L, 0L); , the program header bit will be ignored and fastload will be forced for all programs. arg1 = -1 allows to interrogate the current state of this variable. You need root privileges to toggle the FASTLOAD mode.
| S_SYNCTIME (0x0014) | Allows to interrogate or change the global filesystem sync time. The default value is 5 sec. If arg1 is a positive value, it is interpreted as a new sync time value. If arg1 is equal to -1, the current sync time value will be returned. To be able to change the filesystem sync time you need root privileges desperately.
| S_BLOCKCACHE (0x0015) | A positive value of arg1 ranging from 0 to 100, specifies the percentage of filesystem cache to be filled with linear reads, as in the PERCENTAGE keyword in the mint.cnf file. A negative value of arg1 returns the currently set percentage value. Root privileges are required to use this mode.
| S_FLUSHCACHE (0x0016) | Invalidates CPU cache entries. The arg1 is a pointer to the memory area whose cache entries should be invalidated, the arg2 is the size of the area in bytes. Passing -1 as the arg2 invalidates all cache entries. If the CPU features a separate instruction and data caches, both are flushed. This call automatically recognizes caches in 68020/030/040/060 and handles them as appropriate. The 68060 branch cache is automatically invalidated too. On 68000/68010 calling this mode has no effect. This mode is in fact just an interface to the MiNT function cpush() used internally by the system. Root privileges are NOT required to use this mode.
| S_CTRLCACHE (0x0017) | Provides an universal (among 68k family members) way of controlling the CPU on chip caches. The arg1, referenced as Cache Control Word (CCW) is a bitfield where each bit enables (if 1) or disables (if 0) a particular function of CPU caches. The arg2, referenced as Cache Control Mask (CCM), is a bit mask where you define (by setting appropriate bits to 1) which bits of the Cache Control Word should be actually taken into account and written into the Cache Control Register (CACR). This is control mode of the S_CTRLCACHE. In inquire mode you can pass -1 as either argument. If the CCW is -1, the call returns a longword reflecting the actual state of the caches. If the CCM is -1, a default bitmask is returned, where any bit set indicates, that a cache function defined by the same bit in the Cache Control Word is valid for the processor the MiNT is currently running on. If both arguments are negative, the call simply returns E_OK if it is valid at all or ENOSYS otherwise. This is the acknowledge mode of the S_CTRLCACHE. Bits in either argument are defined as follows:
    0	enable instruction cache
    1	enable data cache
    2	enable branch cache
    3	freeze instruction cache
    4	freeze data cache
    5	instruction burst enable
    6	data burst enable
    7	enable write allocate
    8	instruction cache full mode enable
    9	instruction cache read/write allocate enable
    10	data cache full mode enable
    11	data cache read/write allocate enable
    12	invalidate branch cache
    13	invalidate branch cache user entries
    14	enable CPUSH invalidate
    15	enable store buffer
    16-31	reserved for future definition
Notice, that no processor currently supports all of these functions and some (68000 and 68010) have no on-chip caches at all. To figure out, what functions are valid for the actual CPU used, you should first request the default bitmask using the inquire mode described above. Your program should save this mask, logically AND the arg2 with it, then pass the result as the Cache Control Mask for a control mode call. Also notice, that the above bit definition does not exactly reflect the function and even position of actual bits in the physical Cache Control Register. The bits of either argument are arbitrarily assigned to particular cache functions, but their position and state are converted by the system before the Cache Control Register is written and after it is read, so that the user program can see always the same functions assigned to bits as above regardless of the physical configuration of the Cache Control Register. Since changing cache configuration is global and may severely affect system performance, root privileges are needed to use S_CTRLCACHE control mode.
| S_INITIALTPA (0x0018) | A positive non-zero value of arg1 defines the default amount of memory (in bytes) allocated for TPA space, as in the INITIALMEM keyword of the mint.cnf file. A negative value allows to interrogate the value currently set. A value of 0 is illegal and will cause the call to fail and return EBADARG. Notice that even if you define a very small value, like 1 or 2 bytes, the system will round this up to the smallest size of a memory block possible to allocate. Root privileges are required to use this mode.
| S_CAD (0x0019) | Reserved for future definition.
| S_DELCOOKIE (0x001a) | Removes from the Cookie Jar a cookie, whose tag has been passed as arg1.
| S_LOADKBD (0x001b) | Loads new BIOS keyboard translation table and installs it in the system. The pointer to the keyboards filename should be passed as arg1. Note that this function loads the master translation table, so that after this call succeeds, the Bioskeys() will not be able anymore to restore the previous settings. To restore the real power up defaults you must call this function with NULL passed as arg1.
| S_CLOCKMODE (0x0064) | S_CLOCKMODE called with an arg1 of -1 inquires the kernel's notion of the hardware system clock. If the command returns a zero, the hardware clock is considered to tick in UTC; if it returns a positive non-zero value, it is considered to tick in local time. Any other positive value of the arg1 sets the current clock mode. On a 0 it is reset to UTC, or to local time otherwise. Although this call will never really change the setting of the hardware clock, due to the changed interpretation the clock seems to warp; don't play around too much with it.
| S_KNAME (0x0384) | arg1 and arg2 specify the address and length in bytes, respectively, of a memory buffer, where will be written a NULL terminated ASCII string identifying the full name and version of the system kernel. If the memory buffer is not long enough to hold the entire string, the string is truncated down to the buffer size.
| S_CNAME (0x038e) | arg1 and arg2 specify the address and length in bytes, respectively, of a memory buffer, where will be written a NULL terminated ASCII string identifying the full name of the compiler used to compile the system kernel. If the memory buffer is not long enough to hold the entire string, the string is truncated down to the buffer size.
| S_CVERSION (0x038f) | arg1 and arg2 specify the address and length in bytes, respectively, of a memory buffer, where will be written a NULL terminated ASCII string identifying the version of the compiler used to compile the system kernel. If the memory buffer is not long enough to hold the entire string, the string is truncated down to the buffer size.
| S_CDEFINES (0x0390) | arg1 and arg2 specify the address and length in bytes, respectively, of a memory buffer, where will be written a NULL terminated ASCII string containing the compile time definitions (switches) used while compiling the system kernel. If the memory buffer is not long enough to hold the entire string, the string is truncated down to the buffer size.
| S_COPTIM (0x0391) | arg1 and arg2 specify the address and length in bytes, respectively, of a memory buffer, where will be written a NULL terminated ASCII string containing the compile time optimization options used while compiling the system kernel. If the memory buffer is not long enough to hold the entire string, the string is truncated down to the buffer size.
| S_DEBUGLEVEL (0x03e8) | S_DEBUGLEVEL called with an arg1 of -1 inquires the kernel's current debug level. Any other positive value will set the current debug level. If it is a zero, the kernel will not output any debugging information, except for fatal error messages. The higher the debug level, the more MiNT will spew about what it is doing. Notice, that special debug kernels will output more information than an ordinary distribution kernel. Root privileges are needed to change the debug level.
| S_DEBUGDEV (0x03e9) | S_DEBUGDEV called with an arg1 of -1 inquires the current BIOS device to output the debug information to. The order of defined BIOS devices is as follows: 0, printer 1, AUX: 2, console (default) 3, MIDI 4, keyboard 5, raw screen Any positive value of arg1, that ranges from 0 to 9, will redirect the debug information output to an appropriate BIOS device. Notice however, that setting device 4 (keyboard) as a debug device does not make much sense and may produce undesired results. The system does not restrict this in any way though, just assuming that you know what you're doing. Root privileges are needed to change the debug device.
| S_TIOCMGET (0x54f8) | This mode is reserved for the internal and exclusive usage of the MiNT Library.
Binding |
    move.l  arg2,-(sp)
    move.l  arg1,-(sp)
    move.w	opcode,-(sp)
    move.w  #$0154,-(sp)
    trap    #1
    lea     $0c(sp),sp
Caveats | Ssystem() was first introduced as of MiNT version 1.14.6, but it is considered fully functional as of MiNT version 1.15.0 release. The S_OSHEADER opcode should be only used for fetching the TOS version number when running MiNT versions below 1.15.0 release. The S_FLUSHCACHE, S_CTRLCACHE, S_DEBUGLEVEL and S_DEBUGDEV are supported as of MiNT version 1.15.1 release. You should never use Ssystem(S_TIOCMGET, ...); in own programs. The Ssystem() behaviour does not depend on the S_SECLEVEL settings. Any values returned by the kernel on reserved fields should be considered undocumented and no software should rely on them.
Comments | Its strictly encouraged to access GEMDOS variables and system vectors via the Ssystem(), because this way is considered safe for multiuser setups. For example, you can access the cookie jar pointer using Ssystem(S_GETLVAL, 0x05a0, NULL), though if TOS compatibility is the issue, you should rather use Setexc(0x05a0>>2, -1). Prior to any further Ssystem() usage, your application should first check if the kernel supports this call. If it does, the Ssystem(-1, 0L, 0L); should return a zero. Ssystem() is used and supported by the MiNT Library as of patchlevel 48.
See also | Tgettimeofday(), Tsettimeofday()